{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["船员房间部分"],"not_rendered":{"images":31,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"船员房间部分","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"merged":[[0,0,0,9],[1,0,1,9],[35,0,35,5],[36,0,36,9]],"flags":["formulas_cached_only"]}
["150米三峡游轮船员区家具清单"]
["船名：重轮长江云帆  工程编号：ZJ20-LYC007"]
["序号","家具名称","使用部位","规格尺寸","单位","数量","单价\n（元）","价格\n（元）","参考图片","备注"]
[1,"单人床","船长室","2000*1200*400","张",1,null,0,null,"1.实木框架+实木床板（钢架龙骨增强），软包靠背面料（优质西皮）\n2.甲醛释放量≤0.03mg/m³（国标E1级及以上）\n3.油漆需符合GB 18581-2020，VOC含量≤5g/L\n4.配60椰棕床垫"]
[2,"沙发","船长室","1200*600*400","张",1,null,0,null,"1.框架：实木框架，经过特殊干燥处理，含水率为9~11%，主体采用榫结构，六面抛光，光滑不粗糙。承托力达 150kg；\n2.海绵：高回弹海绵，座垫泡棉密度大于\n40kg/m3，靠背泡棉密度大于25kg/m3，弹性好。表面涂有防止老化变形的保护膜；"]
[3,"茶几","船长室","700*420*450","张",1,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4，实木柱脚或不锈钢柱脚"]
[4,"书桌","船长室","800*550*780","张",1,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[5,"衣柜","驾驶甲板4个/轮机长室/1人间/值班室","800*550*1800","个",10,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[6,"单人床","船员室/值班室","2000*900*400","张",11,null,0,null,"1.实木框架+实木床板（钢架龙骨增强），软包靠背面料（优质西皮）\n2.甲醛释放量≤0.03mg/m³（国标E1级及以上）\n3.油漆需符合GB 18581-2020，VOC含量≤5g/L\n4.配60椰棕床垫"]
[7,"床头柜","船员室/值班室","400*400*450","个",11,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[8,"高低床","船员室","2000*900*2000","张",73,null,0,null,"1.床头架：床立柱50mm×50mm×1.8mm方管，横支撑梁40mm×40mm×1.2mm方管，床头架高度（不含蚊帐架）2110mm，宽度范围900mm。床腿上下两头各加PP工程塑料封口一个, 每组床架含一个人名牌。检测依据：GB 28481-2012《塑料家具中有害物质限量》, 检测结果要求：可溶性重金属检测结果要求4项均未检出。\n2.床层架：架框50mm×25mm×1.5mm扁管，架撑30mm×30mm×1.2mm方管。架长2000mm，架宽900mm。\n3.防护栏板：EO级中纤板EO级刨花板，优质三聚氰胺纸饰面。\n4. 床梯：上落床梯25mm×25mm方管，壁厚1.5mm；\n5 .连接杆：40mm×40mm×1.2mm方管。\n6 .采用δ=20mm优质杉木板，含水率低于14％，经防虫防腐等处理。拼接合缝紧密，长、宽和床层架配套，平整，无空心、无变形、无修补。\n7 .钢管均采用国标无缝管，经防磷除锈处理，表面静电粉末喷涂工艺"]
[9,"阅读桌","船员室/值班室","900*550*780","张",37,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[10,"阅读桌","广播室/上甲监控室","1000*550*780","张",3,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[11,"办公桌","主甲板监控室","1500*600*780","张",1,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[12,"阅读椅","船员室等","厂规（选样）","把",38,null,0,null,"1.面料：优质西皮。具有防污、耐磨、易清洁等特点，机缝线间隙均匀、线条流畅、转角顺畅；\n2.椅脚：白蜡木椅脚，清水油漆\n3.海绵：高回弹海绵，座垫泡棉密度大于\n40kg/m3，靠背泡棉密度大于25kg/m3，弹性好。"]
[13,"衣柜","船员室","900*550*1800","个",85,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n\n\n"]
[14,"会议桌","船长会议室","2600*900*800","张",1,null,0,"=DISPIMG(\"ID_129405EB2BB146379546D17F6B4B1E71\",1)","1、主材：刨花板基材MFC板，欧洲E0级环保标准，甲醛释放量≤0.5mg/L；耐刮损、耐磨性强；封边2mm厚PVC。台面厚度 25mm；\n2、钢脚：50*50方管结构，壁厚2.0mm，表面静电粉末喷涂。\n"]
[15,"会议椅","船长会议室/广播室/监控室","厂规","把",15,null,0,null,"1、面料：优质西皮。具有防污、耐磨、易清洁等特点，机缝线间隙均匀、线条流畅、转角顺畅；\n2、座绵：高密度定型绵，密度约为60g/cm³，回弹性能更佳，座感更加舒适\n3、不锈钢架：304不锈钢管， 钢管Φ25mm，壁厚2.0mm，\n4、净重大于或者等于10.6kg。"]
[16,"沙发","驾驶室","2100*750*450","张",2,null,0,null,"1.面料：优质西皮。具有防污、耐磨、易清洁等特点，机缝线间隙均匀、线条流畅、转角顺畅；\n2.框架：实木内框架，经过特殊干燥处理，含水率为9~11%，主体采用榫结构，六面抛光，光滑不粗糙。承托力达 150kg；\n3.海绵：高回弹海绵，座垫泡棉密度大于\n40kg/m3，靠背泡棉密度大于25kg/m3，弹性好。表面涂有防止老化变形的保护膜；\n 4.不锈钢沙发脚。"]
[17,"文件柜（矮）","驾驶室","1200*400*1100","个",2,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[18,"文件柜（高）","驾驶室","1200*400*1800","个",3,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[19,"高脚椅","驾驶室","400*430*780","把",3,null,0,null,"1.面料：优质西皮。具有防污、耐磨、易清洁等特点，机缝线间隙均匀、线条流畅、转角顺畅；\n2.椅脚：白蜡木椅脚，清水油漆\n3.海绵：高回弹海绵，座垫泡棉密度大于\n40kg/m3，靠背泡棉密度大于25kg/m3，弹性好。"]
[20,"海图桌","驾驶室","1500*900*800","张",1,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[21,"办公桌","驾驶室","1500*800*780","张",2,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[22,"麻将椅","船员活动室","厂规","把 ",12,null,0]
[23,"麻将桌","船员活动室","900*900*780","张",3,null,0]
[24,"茶水柜","船员活动室","1200*400*800","个",1,null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。\n4. 五金配件：优质品牌静音导轨。\n"]
[25,"会议桌","党群活动室","3200*1000*800","张",1,null,0,"=DISPIMG(\"ID_129405EB2BB146379546D17F6B4B1E71\",1)","1、主材：刨花板基材MFC板，欧洲E0级环保标准，甲醛释放量≤0.5mg/L；耐刮损、耐磨性强；封边2mm厚PVC。台面厚度 25mm；\n2、钢脚：50*50方管结构，壁厚2.0mm，表面静电粉末喷涂。\n"]
[26,"会议椅","党群活动室","厂规（选样）","把",11,null,0,null,"1、面料：优质西皮。具有防污、耐磨、易清洁等特点，机缝线间隙均匀、线条流畅、转角顺畅；\n2、座绵：高密度定型绵，密度约为60g/cm³，回弹性能更佳，座感更加舒适\n3、不锈钢架：304不锈钢管， 钢管Φ25mm，壁厚2.0mm，\n4、净重大于或者等于10.6kg。"]
[27,"阅读桌","阅览室","1300*600*780","张",2,null,0,null,"1、主材：刨花板基材MFC板，欧洲E0级环保标准，甲醛释放量≤0.5mg/L；耐刮损、耐磨性强；封边2mm厚PVC。台面厚度 25mm；\n2、钢脚或实木脚：50*50方管结构，壁厚2.0mm，表面静电粉末喷涂。\n"]
[28,"阅读桌","阅览室","800*800*780","张",1,null,0,null,"1、主材：刨花板基材MFC板，欧洲E0级环保标准，甲醛释放量≤0.5mg/L；耐刮损、耐磨性强；封边2mm厚PVC。台面厚度 25mm；\n2、钢脚或实木脚：50*50方管结构，壁厚2.0mm，表面静电粉末喷涂。\n"]
[29,"阅读椅","阅览室","厂规（选样）","把",12,null,0,null,"1.面料：优质西皮。具有防污、耐磨、易清洁等特点，机缝线间隙均匀、线条流畅、转角顺畅；\n2.椅脚：白蜡木椅脚，清水油漆\n3.海绵：高回弹海绵，座垫泡棉密度大于\n40kg/m3，靠背泡棉密度大于25kg/m3，弹性好。"]
[29,"书柜组合（深化确认为准）","阅览室","13000*300*1800","平方",{"v":23.4,"d":"23"},null,0,null,"1. 面材：优质三聚氰胺纸饰面，阻燃、耐磨、耐酸碱、防水。甲醛释放量0.2mg/L\n2. 基材：E0级中纤板、E0级刨花板，甲醛释放量≤5mg/100g，防火、防潮、耐磨、耐酸碱、耐烫、耐污染。\n3. 封边：采用同色PVC封边条，耐干热、耐磨、耐老化。"]
[30,"餐桌","船员餐厅","1200*600*750","张",17,null,0,null,"1、主材：刨花板基材MFC板，欧洲E0级环保标准，甲醛释放量≤0.5mg/L；耐刮损、耐磨性强；封边2mm厚PVC。台面厚度 25mm；\n2、加厚加粗不锈钢柱脚；\n"]
[30,"餐桌","船员餐厅","常规","把",68,null,0,null,"1、主材：刨花板基材MFC板，欧洲E0级环保标准，甲醛释放量≤0.5mg/L；耐刮损、耐磨性强；封边2mm厚PVC。台面厚度 25mm；\n2、加厚加粗不锈钢柱脚；\n"]
["合计（含*%增值税发票）",{"$nulls":6},0]
["注：本次报价需包含运输费，二次转运费，安装人工费，打包费等辅助费用"]